Laweiplein 1

9203 KL Drachten

(0031)(0)512 33 50 00 Reception

(0031)(0)512 33 50 60 Technical department

techniek@lawei.nl

**Studio: technical specifications, measurements and facilities**

**The studio is a ballet rehearsal room with limited technical resources**

**Measurements**

Width 11.80m

Height 4.85m

Depth 12.50m

Stage depth with stand 5.00m

Loading elevator 1.30x2.45x2.09m (w x d x h)

**Soft goods**

Black curtain on rail around the auditorium

The left wall is a mirror with a barre

**Seating**

70 seats: stand with 5 rows on 0, 20, 40 and 60cm

**Lighting**

Roomlights 12x Moodspot, adjustable in 4 rows of 3 lights

Showlights 18x DTS Scena LED 150 PC 8.2-70°

Lighting desk Compulite Spark-top

**Additional lighting**

Par64 CP62

Niethammer HPZ115 1kw 15-38°

Use of additional lighting to be discussed (also used for other halls)

**Power**

Stage right 1x 32 ampère

Stage left 1x 32 ampère

**Sound**

Top 2x Meyer Sound UPA-1P

Sub 2x Meyer Sound 600-HP (t.b.d.)

Processing Galileo 816

Use of desks, monitors and mics to be discussed (also used for other halls)

**Dressing rooms and artist green room**

The Studio is equipped with 2 dressing rooms

Each room includes a private shower and toilet, mirrors with lighting, lockers, a sink

and 4 dressing stations

The artist greenroom is available for eating, drinking and preparing food

You can make use of plates & cutlery, an oven, microwave and an electric stove

There is power available for additional kitchen equipment (32a/380v or 16a/220v)

