Laweiplein 1

9203 KL Drachten

(0031) (0) 512 33 50 00 Reception

(0031) (0) 512 33 50 60 Technical department

techniek@lawei.nl

**Roel Oostrazaal: technical specifications, measurements, facilities.**

**Stage**

Width 14m

Height 12.20m

Depth including proscenium 9.5m

Depth excluding proscenium 6.5m

Depth proscenium 3m

Proscenium arch minimum w x h 8 x 4.75m

Proscenium arch maximum w x h 11 x 4.75m

Best practice width 9m

Orchestra pit no

Firecurtain no

Loading dock Navigation addres: Laweiplein 1

Loading elevator 5.50 x 2.20 x 2.75m (d x w x h)

**Fly bars**

Length 14,5 m

Hand operated bars 28 75kg

Motors 10 200kg

Advance bar 1 250kg

Side fly bars: 2 left and 2 right 4 75kg

**Heights**

Side bridges 7m

Proscenium arch 4.75m

Lowest point wings 3.5m

**Soft goods**

Colour is night blue

4 sets of legs 7 m

3 borders 2.5 m

1 black backdrop on rail

1 white backdrop

1 black gauze

1 night blue drop

**Seating**

Front auditorium 207

Rear auditorium 151 There is a division curtain

Wheelchair 8

Balcony 114

**Lighting**

Hall catwalk 15x 2 kw Niethammer zoomprofile HPZ 215 15-40°

Coves per side 2x 2 kw Niethammer zoomprofile HPZ215 15-40°

Portal 8x 2 kw ADB PC 8-48°

 6x 1 kw Niethammer zoomprofile HPZ 115 15-38°

Under portal 5x 1 kw Strand PC

Manteau per side 2x 1 kw Niethammer zoomprofile HPZ 115

2x 1 kw Strand PC

Horizon 5x 4 colours 1 kw

Lighting deskCompulite Spark-top

**Additional lighting**

Sixbar PAR64 CP62 4

Par64 CP62 8

1 kw Niethammer HPZ115 6 15-38°

1 kw Selecon PC 10

Use of additional lighting to be discussed (also used for other halls)

**Power**

Stageright 1x 32 ampère/380 volts

Stageleft 1x 63 ampère/380volts

**Sound**

**Room system** Acoustic Line

Main PA 2x CT 12 per side

Center 2x CT 12

Sub 2x CB 215

Processing Xilica XP 4080

Inputs L/R, L/R/sub, L/R/center or L/R/center/sub

**Monitor\***

KS audio passive monitors: 10 inch, 12 inch en 15 inch

**Sounddesk\***

Analog Midas VeniceF 24 ch, Soundcraft M4 en M8

Digital Allen&Heath QU-16, Midas Pro2c, Yamaha LS9

**Microphones wireless\***

8x Sennheiser EW300 G3 Frequency range B 626-668

8x e865 Handheld

8x SK300 Beltpack

4x DPA d:fine

6x DAP EH 2

2x Sennheiser MKE2 black

**Microphones and DI’s\***

Shure SM52b, SM56b, SM57, SM57b, SM58, SM58b, SM87, SM91b

Sennheiser 421, e604, e906, ME35, ME66, MD 808-U

Neumann KM184, KMS105

AKG C214B, C414B, C452 EB, D112

Radial J48, JDI Duplex

Klark Teknik DN100

Arx Audibox usb DI

**\***Use of desks, monitors and mics to be discussed (also used for other rooms)

**Dressing rooms and artist green room**

The Roel Oostrazaal is equipped with 4 dressing rooms, one featuring a private shower and toilet

For the other rooms showers and toilets are close by

Each room includes mirrors with lighting, lockers, a sink and 4 to 8 dressing stations

The artist greenroom is available for eating, drinking and preparing food

You can make use of plates & cutlery, an oven, microwave and an electric stove

There is power available for additional kitchen equipment (32a/380v or 16a/220v)